**SECTION – F**

**STANDARD DETAILS INDEX**

**Issue Date: June 2020**

# Standard Detail Index

|  |  |
| --- | --- |
| **Drawing**  **Number** | **Details** |
| 101 | Turning Areas – Residential Streets |
| 102 | Turning Areas – Mews Court |
| 103 | Turning Area – Industrial and Commercial |
| 104 | Private Shared Access Serving up to 5 Dwellings |
| 105 | Turning Areas Private Shared Access (in excess of 45m) |
| 106 | Forward Visibility Envelopes |
| 107 | Arrangement of Passing Bays Roads Less Than 5.5m |
| 108 | Uncontrolled Pedestrian Crossing |
| 109 | Controlled Pedestrian Crossing |
| 110 | Controlled Staggered Pedestrian Crossing |
| 111 | Junction Plateau Raised Carriageway Layout |
| 112 | Junction Plateau Kerbing |
| 113 | Mini Roundabout |
| 114 | Roundabout |
| 115 | Junction Road Markings |
| 116 | Junction Road Markings – Junctions with Primary Roads |
| 117 | Pedestrian and Cycle Staggered Barrier |
| 118 | Disabled Parking Bay Arrangement |
| 119 | Parking Arrangement Public Highway |
| 120 | Parking Arrangement Carparks |
| 121 | Parking Standards |
|  |  |
| 201 | Footway and Carriageway Construction Residential Streets |
| 202 | Vehicle Crossover Residential Streets |
| 203 | Grit and Salt Bin Hardstanding |
| 204 | Mews Court Carriageway, Footway and Vehicle Crossover |
| 205 | Mews Court Rumble Strip |
| 206 | Mews Court Kerb |
| 207 | Mews Court Block Paving Pattern and Colour |
| 208 | Mews Court Block Paving Pattern & Gully Frame Setting |
| 209 | Block Paved Vehicle Crossover |
| 210 | Shared Surface Construction |
| 211 | Shared Surface Construction and Drainage Arrangements |
| 212 | Footway and Carriageway Construction for Residential Streets (Bus Routes) |
| 213 | Ramp Detail for Raised Carriageway |
|  |  |
| **Drawing**  **Number** | **Details** |
|  |  |
| 214 | Ramp Construction Detail –Raised Carriageway- Macadam Plateau |
| 215 | Ramp Construction Detail –Raised Carriageway- Bus Route |
| 216 | Ramp Construction Detail –Raised Carriageway- Macadam Ramp and Plateau |
| 217 | Rumble Strip |
| 218 | Shared and Segregated Footway and Cycleway |
| 219 | Shared Cycle Footpath and Bridleway |
| 220 | Block Paved Awareness Surfacing |
| 221 | Back Lane Construction |
| 222 | External Wall Insulation Abutting Highway |
|  |  |
| 301 | Footway & Carriageway Construction Industrial Estate & Commercial Roads |
| 302 | Footway & Vehicle Crossover Industrial Estate and Commercial Roads |
|  |  |
| 401 | Bus Bays |
| 402 | Bus Stop |
| 403 | Bus Stop Construction |
| 404 | Pedestrian Guardrail |
| 405 | Pedestrian Guardrail (Visirail) |
| 406 | Pedestrian Guardrail (Kee Klamp) |
| 407 | Group P2 Vertical Infill Vehicle Pedestrian Parapet (48kph Traffic Speed) |
| 408 | Precast Concrete Kerbs and Edgings |
| 409 | Trief Kerbing |
| 410 | Kassel Kerbing |
| 411 | Round Top Road Hump and Road Markings |
| 412 | Flat Top Road Hump and Road Markings |
| 413 | Speed Cushions and Road Markings |
| 414 | Speed Cushion Construction |
| 415 | Street Nameplate |
| 416 | Arrangement of Services in Footway |
| 417 | Tie-in of Existing with New Carriageway Construction |
| 418 | Public Stairway |
| 419 | Grass Paving |

|  |  |
| --- | --- |
| **Drawing**  **Number** | **Details** |
|  |  |
| 501 | Manhole Detail Type A Depth to Soffit 3m-6m |
| 502 | Manhole Detail Type B Maximum Depth to Soffit 3m |
| 503 | Manhole Detail Type C Depth to Soffit 1m-1.5m |
| 504 | Manhole Detail Type D Depth to Soffit <1m |
| 505 | Manhole Details Types E Depth to Soffit 1m-1.45m & Type F Depth to Soffit <1m |
| 506 | Flow Control Chamber and Weir Wall |
| 507 | Vertical Backdrop |
| 508 | Short Length Pipe and Rocker Pipe |
| 509 | Chamber Size & Drainage Notes |
| 510 | Precast Concrete Gully |
| 511 | Brick Road Gully & Footway Gully |
| 512 | Trench Bedding and Flexible Joint |
| 513 | Lined Ditch and Outfall |
| 514 | Trash Screen |
| 515 | Soakaway |
| 516 | Pre-cast Concrete Catchpit |
| 517 | Stone Lined Ditch |
| 518 | Filter Drain |
| 519 | Silt Gravel Trap |
| 520 | Silt Gravel Trap – Grid |
|  |  |
| 601 | Concrete Retaining Wall 0.9m – 1.2m |
| 602 | Concrete Retaining Wall 1.5m |
| 603 | Concrete Retaining Wall 1.8m – 3m |
| 604 | Reinforced Concrete T Cantilever Wall |
| 605 | Masonry Gravity Wall 0.9m |
| 606 | Masonry Gravity Wall 1.4m – 1.7m |
| 607 | Masonry Gravity Wall 2m |
| 608 | Pocket Type Reinforced Masonry Wall |
| 609 | Reinforced Grouted Masonry Wall |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| **Drawing**  **Number** | **Details** |
|  |  |
| 701 | Aluminium Lighting Column |
| 702 | Column Identification Plate |
| 703 | Bracket Assembly to Attach Sign to Lighting Column or Structure |
| 704 | Sign Post - Non Illuminated |
| 705 | Sign Post Single - Illuminated |
| 706 | Sign Post Foundation Details for Two and Three Post Sign Assemblies |
| 707 | Zebra Crossing Post and 24V LED Beacon |
| 708 | Wiring Diagram 1. Cut Out to Harvard Leaf Nut - WPD PME Service |
| 709 | Wiring Diagram 2.Cut Out to Harvard Leaf Nut - Authority Supply |
| 710 | Harvard Leafnut Section 38 Guide |
| 711 | Eight (8) Way Stainless Steel or Galvanised Feeder Pillar |
| 712 | Street lighting Feeder Pillar General Arrangement |
| 713 | Arrangement of Street Lighting Apparatus |
| 714 | Cross Section of Street Lighting Duct in Footway |
| 715 | Cross Section of Street Lighting Duct in Carriageway |
| 716 | Access Chamber – Street Lighting Duct in Footway |
| 717 | Access Chamber – Street Lighting Duct in Carriageway |
| 718 | Service Ducts and Reinstatement in Tarmacadam Carriageways and Footways |
| 719 | Service Ducts and Reinstatement in Paved Footways and Verges |
| 720 | Earth Electrode Pit |
| 721 | Street Lighting Column, Access Chamber and Earth Electrode in Highway Verge |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |